NURAJACK  
TECHNICAL DATA SHEET

# PRODUCT DETAILS

|  |  |
| --- | --- |
| Product Description | Nurajacks are an adjustable, self-levelling pedestal support system for tile, paving or timber decking over exterior membrane waterproofing. The system consists of:   * Nurajack Adjustable pedestal with self-levelling head in multiple sizes from 28mm to 550mm * Nurajack Star.t and Nurapad offer low profile solutions starting from 8mm in height * Accessories include: - Nuragrid  - Tile Cladding Clip (5mm, 10mm, 15mm, 20mm) for use  between wall/balustrade and tile/paver   - Adjustment Key  - Shims (1mm, 2mm or 3mm)  For a full list of accessories, visit www.nurajack.co.nz. |
| Scope of use | Nurajacks can be used within the scope of NZBC E2/AS1.  Nurajacks can be installed over Concrete, Ply or Enertherm insulated substrates with a membrane. Nurajacks can also be installed over concrete patio or other suitable substrates to facilitate level threshold doorways.  Nurajacks are compatible with all sheet membranes (eg. Butyl, TPO, Bitumen etc.) and are installed without penetration of the membrane.  Nurajacks are suitable for new or existing commercial and residential buildings. |

|  |  |
| --- | --- |
| Company Name | **Nuralite Waterproofing Ltd** |
| Contact name & details | Lewis Olding Nuralite waterproofing Ltd 60D Leon Leicester Ave Mt Wellington  Auckland ph (09) 579 2046 |
| Product names/Name of PTS | Nurajack SE  Nurajack Star.T  Nurapad  Nurapad Shim  Nuragrid |
| Level of assurance which is met by |  |

|  |  |
| --- | --- |
| In service history (NZ & overseas) | 1000’s of residential and commercial projects around New Zealand. Some examples include:   * Sugar Tree Apartments Auckland * Sky City Auckland * Heritage Hotel Auckland * Taupo Water Treatment Plant * National Library Wellington |

|  |  |
| --- | --- |
| New Zealand Building Code | New Zealand Building Code Clause E2 Pages 54 & 55  Codemark BCS-151216-CMNZ |

Conditions

|  |  |
| --- | --- |
| Design guidelines | * Tiled and Timber decks must be enclosed with a parapet or balustrade. * See [www.nurajack.co.nz/downloads](http://www.nurajack.co.nz/downloads) for detail drawings and specifications. |
| Installation requirements | See [www.nurajack.co.nz](http://www.nurajack.co.nz) for full installation details. |
| Maintenance requirements | Periodic checking for loose Nurajacks especially if the substrate has moved. |
| Warranty | 20-year product warranty. |

Other company information

|  |  |
| --- | --- |
| Environmental | ISO 14001, LEED Credits |
| Quality assurance |  |
| Groups company is a member of |  |

Sign off:

The information above is true and accurate. All test results are available upon request and I have not withheld anything that could result in the product complying with the identified performance clauses of the NZ building code.

A close-up of a black wire

AI-generated content may be incorrect.Nuralite Waterproofing Ltd. accepts any and all liability arising from reliance upon the information contained in this document and replicated on the Masterspec PTS template.

Signed:

Title: Managing Director

The information in this product data sheet is based on our experience and testing. It represents the latest information available at the time of printing, but no guarantee of its accuracy is made or implied, nor responsibility taken for use to which this information may be put.   
We reserve the right to alter or up-date information parameters and formulations at any time without notice.